
<----------
INVITE

----------
set_Variable=route1 "Record-Route-1:" "*"

----------
set_Variable=route2 "Record-Route-2:" "*"

----------
set_Variable=route3 "Record-Route-3:" "*"

---------->
SIP/2.0 100 Trying
[last_Via:]
[last_From:]
[last_To:]
[last_Call-ID:]
[last_CSeq:]
User-Agent: SIPInspector_v_[ver]
Content-Length: 0


---------->
SIP/2.0 180 Ringing
[last_Via:]
[last_From:]
[last_To:];tag=[call_number]
[last_Call-ID:]
[last_CSeq:]
Contact: <sip:[local_ip]:[local_port];transport=[transport]>
User-Agent: SIPInspector_v_[ver]
Content-Length: 0


---------->
SIP/2.0 200 OK
[last_Via:]
[last_From:]
[last_To:];tag=[call_number]
[last_Call-ID:]
[last_CSeq:]
Record-Route: <sip:route3@10.11.12.13:41956;lr>
Record-Route: <sip:route2@192.168.1.100:51519;lr>
Record-Route: <sip:route1@[local_ip]:[local_port];lr>
Contact: <sip:[local_ip]:[local_port];transport=[transport]>
User-Agent: SIPInspector_v_[ver]
Content-Type: application/sdp
Content-Length: [len]

v=0
o=111 843670094 843670094 IN [IP_ver] [local_ip_sdp]
s=-
c=IN [IP_ver] [local_ip_sdp]
t=0 0
a=sendrecv
m=audio [media_port] RTP/AVP 0 101
a=rtpmap:0 PCMU/8000
a=rtpmap:101 telephone-event/8000
a=fmtp:101 0-15
a=ptime:20

<----------
ACK

----------
cmd_Pause=1000

---------->
BYE sip:[toUsername]@[remote_ip]:[remote_port];transport=[transport] SIP/2.0
Via: SIP/2.0/[transport] [local_ip]:[local_port];branch=[branch]
From: <sip:[fromUsername]@[local_ip]:[local_port]>;tag=[call_number]
To: <sip:[toUsername]@[remote_ip]:[remote_port]>;[peer_tag_param]
Call-ID: [call_number]@[local_ip]
CSeq: [cseq+1] BYE
Max-Forwards: 70
Route: [$route1]
Route: [$route2]
Route: [$route3]
Contact: <sip:[fromUsername]@[local_ip]:[local_port];transport=[transport]>
User-Agent: SIPInspector_v_[ver]
Content-Length: 0


<----------
200 OK
