
---------->
INVITE sip:[field1]@[remote_ip]:[remote_port] SIP/2.0
Via: SIP/2.0/[transport] [local_ip]:[local_port];branch=[branch]
From: <sip:[field0]@[local_ip]:[local_port]>;tag=[call_number]
To: <sip:[field1]@[remote_ip]:[remote_port]>
Call-ID: 4fun[call_number]@[local_ip]
CSeq: [cseq+1] INVITE
Max-Forwards: 70
Contact: <sip:[field0]@[local_ip]:[local_port];transport=[transport]>
User-Agent: SIPInspector_v_[ver]
Content-Type: application/sdp
Content-Length: [len]

v=0
o=111 843670094 843670094 IN [IP_ver] [local_ip_sdp]
s=-
c=IN [IP_ver] [local_ip_sdp]
t=0 0
a=sendrecv
m=audio [media_port] RTP/AVP 0 8 18 101
a=rtpmap:0 PCMU/8000
a=rtpmap:8 PCMA/8000
a=rtpmap:18 G729/8000
a=rtpmap:101 telephone-event/8000
a=fmtp:101 0-15
a=ptime:20

<----------*
100 Trying

<----------
407 Proxy Authentication Required

---------->
ACK sip:[field1]@[remote_ip]:[remote_port];transport=[transport] SIP/2.0
Via: SIP/2.0/[transport] [local_ip]:[local_port];branch=[branch]
From: <sip:[field0]@[remote_ip]:[remote_port]>;tag=[call_number]
To: <sip:[field1]@[remote_ip]:[remote_port]>;[peer_tag_param]
Call-ID: 4fun[call_number]@[local_ip]
CSeq: [cseq] ACK
Max-Forwards: 70
Contact: <sip:[field0]@[local_ip]:[local_port];transport=[transport]>
User-Agent: SIPInspector_v_[ver]
Content-Length: 0


---------->
INVITE sip:[field1]@[remote_ip]:[remote_port];transport=[transport] SIP/2.0
Via: SIP/2.0/[transport] [local_ip]:[local_port];branch=[branch]ab
From: <sip:[field0]@[remote_ip]:[remote_port]>;tag=[call_number]
To: <sip:[field1]@[remote_ip]:[remote_port]>
Call-ID: 4fun[call_number]@[local_ip]
CSeq: [cseq+1] INVITE
Max-Forwards: 70
Contact: <sip:[field0]@[local_ip]:[local_port];transport=[transport]>
User-Agent: SIPInspector_v_[ver]
Proxy-Authorization: [authentication username=[field2]; password=[field3];]
Content-Type: application/sdp
Content-Length: [len]

v=0
o=111 843670094 843670094 IN [IP_ver] [local_ip_sdp]
s=-
c=IN [IP_ver] [local_ip_sdp]
t=0 0
a=sendrecv
m=audio [media_port] RTP/AVP 0 8 18 101
a=rtpmap:0 PCMU/8000
a=rtpmap:8 PCMA/8000
a=rtpmap:18 G729/8000
a=rtpmap:101 telephone-event/8000
a=fmtp:101 0-15
a=ptime:20

<----------*
100 Trying

<----------
180 Ringing

<----------
200 OK

---------->
ACK sip:[field1]@[remote_ip]:[remote_port] SIP/2.0
Via: SIP/2.0/[transport] [local_ip]:[local_port];branch=[branch]
From: <sip:[field0]@[local_ip]:[local_port]>;tag=[call_number]ac
To: <sip:[field1]@[remote_ip]:[remote_port]>;[peer_tag_param]
Call-ID: 4fun[call_number]@[local_ip]
CSeq: [cseq] ACK
Max-Forwards: 70
Contact: <sip:[field0]@[local_ip]:[local_port];transport=[transport]>
User-Agent: SIPInspector_v_[ver]
Content-Length: 0


----------
cmd_PlayPcap=.\pcap\test.pcap

----------
cmd_Pause=15000

---------->
BYE sip:[field1]@[remote_ip]:[remote_port] SIP/2.0
Via: SIP/2.0/[transport] [local_ip]:[local_port];branch=[branch]cd
From: <sip:[field0]@[local_ip]:[local_port]>;tag=[call_number]
To: <sip:[field1]@[remote_ip]:[remote_port]>;[peer_tag_param]
Call-ID: 4fun[call_number]@[local_ip]
CSeq: [cseq+1] BYE
Max-Forwards: 70
Contact: <sip:[field0]@[local_ip]:[local_port];transport=[transport]>
User-Agent: SIPInspector_v_[ver]
Content-Length: 0


<----------
200 OK
