
---------->
REGISTER sip:[remote_ip]:[remote_port] SIP/2.0
Via: SIP/2.0/[transport] [local_ip]:[local_port];branch=[branch]
From: <sip:[fromUsername]@[remote_ip]:[remote_port]>;tag=24de4a5dbe4ef
To: <sip:[fromUsername]@[remote_ip]:[remote_port]>
Call-ID: [call_number]@[local_ip]
CSeq: [cseq] REGISTER
Expires: 3600
Max-Forwards: 70
Contact: <sip:[fromUsername]@[local_ip]:[local_port];transport=[transport]>
User-Agent: SIPInspector_v_[ver]
Content-Length: 0


<----------*
100 Trying

<----------*
401 Unauthorized

---------->*
REGISTER sip:[remote_ip]:[remote_port] SIP/2.0
Via: SIP/2.0/[transport] [local_ip]:[local_port];branch=[branch]
From: <sip:[fromUsername]@[remote_ip]:[remote_port]>;tag=24417923471779367133
To: <sip:[fromUsername]@[remote_ip]:[remote_port]>;ta
Call-ID: [call_number]@[local_ip]
CSeq: [cseq+1] REGISTER
Max-Forwards: 70
Expires: 3600
Contact: <sip:[fromUsername]@[local_ip]:[local_port];transport=[transport]>
User-Agent: SIPInspector_v_[ver]
Authorization: [authentication username=[authUsername]; password=[authPassword];]
Content-Length: 0


<----------
200 OK

---------->
INVITE sip:[toUsername]@[remote_ip]:[remote_port] SIP/2.0
Via: SIP/2.0/[transport] [local_ip]:[local_port];branch=[branch]
From: <sip:[fromUsername]@[local_ip]:[local_port]>;tag=24417923471779367133
To: <sip:[toUsername]@[remote_ip]:[remote_port]>
Call-ID: [call_number]@[local_ip]
CSeq: [cseq+1] INVITE
Max-Forwards: 70
Contact: <sip:[fromUsername]@[local_ip]:[local_port];transport=[transport]>
User-Agent: SIPInspector_v_[ver]
Content-Type: application/sdp
Content-Length: [len]

v=0
o=111 843670094 843670094 IN [IP_ver] [local_ip_sdp]
s=-
c=IN [IP_ver] [local_ip_sdp]
t=0 0
a=sendrecv
m=audio [media_port] RTP/AVP 8 101
a=rtpmap:8 PCMA/8000/1
a=rtpmap:101 telephone-event/8000
a=fmtp:101 0-15
a=ptime:20

<----------*
100 Trying

<----------
407 Proxy Authentication Required

---------->
ACK sip:[toUsername]@[remote_ip]:[remote_port];transport=[transport] SIP/2.0
Via: SIP/2.0/[transport] [local_ip]:[local_port];branch=[branch]ab
From: <sip:[fromUsername]@[remote_ip]:[remote_port]>;tag=24417923471779367133
To: <sip:[toUsername]@[remote_ip]:[remote_port]>;[peer_tag_param]
Call-ID: [call_number]@[local_ip]
CSeq: [cseq] ACK
Max-Forwards: 70
Contact: <sip:[fromUsername]@[local_ip]:[local_port];transport=[transport]>
User-Agent: SIPInspector_v_[ver]
Content-Length: 0


---------->
INVITE sip:[toUsername]@[remote_ip]:[remote_port];transport=[transport] SIP/2.0
Via: SIP/2.0/[transport] [local_ip]:[local_port];branch=[branch]
From: <sip:[fromUsername]@[remote_ip]:[remote_port]>;tag=24417923471779367133
To: <sip:[toUsername]@[remote_ip]:[remote_port]>
Call-ID: [call_number]@[local_ip]
CSeq: [cseq+1] INVITE
Max-Forwards: 70
Contact: <sip:[fromUsername]@[local_ip]:[local_port];transport=[transport]>
User-Agent: SIPInspector_v_[ver]
Proxy-Authorization: [authentication username=[authUsername]; password=[authPassword];]
Content-Type: application/sdp
Content-Length: [len]

v=0
o=111 843670094 843670094 IN [IP_ver] [local_ip_sdp]
s=-
c=IN [IP_ver] [local_ip_sdp]
t=0 0
a=sendrecv
m=audio [media_port] RTP/AVP 8 101
a=rtpmap:0 PCMA/8000/1
a=rtpmap:101 telephone-event/8000
a=fmtp:101 0-15
a=ptime:20

<----------*
100 Trying

<----------*
180 Ringing

<----------*
183 Session Progress

<----------
200 OK

----------
set_Variable=toTag "To:" "tag=*"

----------
set_Variable=recRoute "Record-Route:" "*"

----------
set_Variable=remContact "Contact:" "<*>"

---------->
ACK [$remContact] SIP/2.0
Via: SIP/2.0/[transport] [local_ip]:[local_port];branch=[branch]cd
From: <sip:[fromUsername]@[local_ip]:[local_port]>;tag=24417923471779367133
To: <sip:[toUsername]@[remote_ip]:[remote_port]>;tag=[$toTag]
Call-ID: [call_number]@[local_ip]
Route: [$recRoute]
CSeq: [cseq] ACK
Max-Forwards: 70
Contact: <sip:[fromUsername]@[local_ip]:[local_port];transport=[transport]>
User-Agent: SIPInspector_v_[ver]
Content-Length: 0


----------
cmd_PlayPcap=.\pcap\711aLaw.pcap

----------
cmd_Pause=15000

---------->
INVITE [$remContact] SIP/2.0
Via: SIP/2.0/[transport] [local_ip]:[local_port];branch=[branch]ef
From: <sip:[fromUsername]@[remote_ip]:[remote_port]>;tag=24417923471779367133
To: <sip:[toUsername]@[remote_ip]:[remote_port]>;tag=[$toTag]
Call-ID: [call_number]@[local_ip]
CSeq: [cseq+1] INVITE
Max-Forwards: 70
Route: [$recRoute]
Contact: <sip:[fromUsername]@[local_ip]:[local_port];transport=[transport]>
User-Agent: SIPInspector_v_[ver]
Content-Type: application/sdp
Content-Length: [len]

v=0
o=111 843670094 843670096 IN [IP_ver] [local_ip_sdp]
s=-
c=IN [IP_ver] [local_ip_sdp]
t=0 0
a=sendrecv
m=audio [media_port] RTP/AVP 9 101
a=rtpmap:9 G722/8000/1
a=rtpmap:101 telephone-event/8000
a=fmtp:101 0-15
a=ptime:20

<----------*
100 Trying

<----------
200 OK

---------->
ACK [$remContact] SIP/2.0
Via: SIP/2.0/[transport] [local_ip]:[local_port];branch=[branch]gh
From: <sip:[fromUsername]@[remote_ip]:[remote_port]>;tag=24417923471779367133
To: <sip:[toUsername]@[remote_ip]:[remote_port]>;tag=[$toTag]
Call-ID: [call_number]@[local_ip]
Route: [$recRoute]
CSeq: [cseq] ACK
Max-Forwards: 70
Contact: <sip:[fromUsername]@[local_ip]:[local_port];transport=[transport]>
User-Agent: SIPInspector_v_[ver]
Content-Length: 0


----------
cmd_PlayPcap=F:\Projects\SIPInspector\pcap\722.pcap

----------
cmd_Pause=15000

---------->
BYE sip:[toUsername]@[remote_ip]:[remote_port] SIP/2.0
Via: SIP/2.0/[transport] [local_ip]:[local_port];branch=[branch]ij
From: <sip:[fromUsername]@[local_ip]:[local_port]>;tag=24417923471779367133
To: <sip:[toUsername]@[remote_ip]:[remote_port]>;tag=[$toTag]
Call-ID: [call_number]@[local_ip]
CSeq: [cseq+1] BYE
Max-Forwards: 70
Contact: <sip:[fromUsername]@[local_ip]:[local_port];transport=[transport]>
User-Agent: SIPInspector_v_[ver]
Content-Length: 0


<----------
200 OK
